XUIMSThe X-Window User Interface Management System at CERNM.Vanden Eynden (E-mail : veym@dxcern.cern.ch)CERN SL Controls GroupEuropean Laboratory for Particle PhysicsCH 1211 Geneva 23, SwitzerlandABSTRACTThe CERN X-Window User Interface Management System (XUIMS) is a modular and highly configurable softwaredevelopment environment allowing the interactive design, prototyping, and production of OSF/Motif Human ComputerInterfaces (HCI). Fully compliant with the X11R5 and OSF/Motif industry standards, XUIMS covers complex softwareareas like the development of schematics, the visualization and on-line interactions with 2D and 3D scientific data, thedisplay of relational database data and the direct access to CERN SPS and LEP accelerator equipment.The guarantee of consistency across the applications and the encapsulation of complex functionality in re-usable and user-friendly components has also been implemented through the development of home made graphical objects (widgets) andtemplates.The XUIMS environment is built with commercial software products integrated in the CERN SPS and LEP controlsinfrastructure with a very limited in-house effort.Productivity and quality have been improved through less coding and better HCI prototyping.INTRODUCTIONThe X-Window and OSF/Motif industry standards have been used since 1992 to produce the Human Computer Interfaces(HCI) required for the control of the two CERN largest particle accelerators : SPS and LEP. The decision to base the HCIsoftware activity on industry standards was made to avoid, as much as possible, vendor-specific developments and toguarantee thereby the software investment for a long time [1].The desire to optimize the production of HCIs led to several market investigations and product evaluations. In 1994, acommercial User Interface Management System was selected to become the kernel of the CERN X-Windows User InterfaceManagement System (XUIMS) [2].X-WINDOWS AND OSF/MOTIF The X-Windows and OSF/Motif software market has rapidly evolved during last two years and today offers a large choice ofHCI software development environments. One could still consider the development of HCIs using only the standard X-Window and OSF/Motif libraires, but if a higher degree of abstraction and reusability is required, or if special features (i.e.2D and 3D scientific data visualization) are needed, then using a powerful software development environment becomesmandatory. The next four sections summarise the different strategies that can be considered for the developement ofOSF/Motif interfaces.X-WINDOWS AND OSF/MOTIF LIBRARIESThe X-Windows and OSF/Motif libraries (Xlib, XtIntrinsics, and Xm) are intended to be called from a C application andcontain low level functions for the creation and manipulation of HCI components (i.e. buttons, labels and lists of elements).Any modification in the HCI requires a change in the C program (i.e. editing, compilation, and debugging developmentcycle). The final HCI C code is not understandable by any Interface Development Tool (IDT) or User Interface ManagementSystem (UIMS) and has therefore to be maintained manually.

OSF/MOTIF USER INTERFACE LANGUAGEThe OSF/Motif UIL language is a specification language for describing the initial state of a user interface for a Motifapplication. The specification describes the objects (i.e. menus, form boxes and buttons) used in the interface and specifiesthe functions to be called when the interface changes state as a result of user interaction. The main advantage of UIL is thatit is understood by most IDTs and UIMSs. Nevertheless, UIL does not address the dynamic aspects of the interface (i.e.printing an information message when the user presses a button) and still requires the recompilation of the UIL file aftereach modification.INTERFACE DEVELOPMENT TOOLSStandard Interface Development Tools (IDT) help the developer to design the layout of the interface through a What YouSee Is What You Get (WYSIWYG) interface and to generate the corresponding C code. The application code has then to beinserted into stubs. The main disadvantage of the IDT is that the HCI behavior (i.e putting an alarm message on the screen)must still be handled by the application code, leading to non-reusable software (see chapter about HCI developmentprinciples).USER INTERFACE MANAGEMENT SYSTEMSUser Interface Management Systems (UIMS) add to the IDT functionality the possibility to design and prototype thedynamic behavior of the HCI. These tools can usually import UIL files and export UIL, C, or C++ HCI code. Their abilityto address both the static and dynamic aspects of the HCI offers for the first time the possibility to put in place a real HCIsoftware development lifecycle policy.These considerations led us to buy a commercial UIMS and to enrich it with :• new HCI components such as 2D and 3D graphics widgets,• additional high level C functions (i.e. routines for direct SPS and LEP equipment access),• templates for a common style and behaviour within the SPS and LEP operational environment.THE XUIMS ARCHITECTUREAs shown in Fig 1, XUIMS is a highly modular and configurable environment composed of the following building blocks :• The XFaceMakerTM UIMS. XFaceMaker[3] has a WYSIWYG editor for the interactive creation of HCI layouts.Fig 1 : The XUIMS Architecture XFaceMaker UIMSXDrawMakerXRT WidgetsXuims WidgetsXuims TemplatesXuims Library Xuims DB

The HCI behavior is specified in the form of procedural scripts in a high-level, C-like programing language calledFACE. The behavior can be tested within the tool using the built-in interpreter and debugger for the FACE scriptinglanguage. C, C++, and UIL code are generated by the tool. Additional C libraries can be linked into the UIMS kernel(i.e. libraries for SPS and LEP accelerator equipment access) in order to extend the basic functionalities of XFaceMaker.Working HCIs produced with XFaceMaker can run on any workstation without run-time fees (this is also the case forthe other commercial products used in XUIMS). XFaceMaker also allows the programmer to define templates (compositeobjects) and to add new widgets to the standard OSF/Motif widgets set. • The XDrawMakerTM drawing package. XDrawMaker [4] is a drawing editor enhanced by the ability to animate objects.When used with XFaceMaker, every object becomes a widget that can be included and manipulated in the HCI. Attributesof objects in complex schematics (see Fig 2) can be handled as any standard OSF/Motif widget. Almost any imaginabletask can be handled with XDrawMaker.Title:xuimssynCreator:xgrabscCreationDate:TueOct1011:11:531995Fig 2 : Schematics of CERN�s intricate particle beam network built with XDrawMaker. Courtesy of the CERN SL Transfer Line project team. • The XRTTM 2D, 3D and Table widgets. The XRT/2D widget can display virtually any type of two-dimensional graph,including barcharts, X-Y plots, pie charts, area graphs and logarithmic scientific charts. The XRT/3D widget can contourand zone 3D data. Users can dynamically rotate, zoom and scale views. The XRT/table widget allows developers todisplay and manipulate tabular data. The XRT widgets were selected for their excellent real-time performance. Fig 3shows Xplore, the CERN off-line scientific data visualization package built with XUIMS and the XRT/2D widget. • The XUIMS library. This C libary contains additional functions used for direct access to the SPS and LEP acceleratorsequipment, for direct access to the UNIX file system, for providing on-line hypertext help on the WWW and for thehandling of HCI components (i.e. flashing widgets, information messages, and cursor manipulations). • The XUIMS widgets. Extending the OSF/Motif widgets set with XFaceMaker is a trivial exercise. New widgets andtheir associated code can be developed interactively with the WYSIWYG editor and added to the standard paletteafterwards. This important feature has been used to create additional widgets for formatted numeric entries, for fileprinting and screen dumping and for providing help. • The XUIMS templates. As shown in Fig 3, a template is a model, defined by a pre-designed object, that can be appliedto other objects, called the instances of the template, which inherit the attributes defined in the template. A template canalso be a composite object (i.e. a main window with predefined buttons and actions). Templates are very useful toencapsulate high-level functionality in a reusable way and to enforce consistency across the applications.

Title:xuims2dCreator:xgrabscCreationDate:MonOct916:33:541995 Fig 3 : The CERN Xplore off-line scientific data visualization Package built with the XUIMS 2D template. • The XUIMS resources database. The main purpose of this database is to guarantee a standard behavior for all X-Windowsapplications running in the SPS and LEP control room. Consistency is important both between applications and withina single application. Consistency helps the user to transfer familiar skills to new situations. The user can apply theknowledge learned from one application to another application, reducing the amount of learning and subsequent calls (i.e.an operator will easily recognize a push-button in an application if all pushbuttons have the same background andforeground colors). A primary XUIMS resources database [5] contains low priority definitions of resource values (i.e.fonts and colors) affecting all X-Window HCIs. If needed, a secondary resource database containing higher priorityresource values can be provided by the developer for one given HCI.THE HCI DESIGN WITH XUIMSTHE INTERFACE AND THE APPLICATIONThe fundamental principle of HCI software development is the separation between the application and the interface [6].The application can be seen as the set of routines and algorithms specific to the process or equipment to be controlled (i.e.routine for switching a vacuum pump ON and OFF). The interface can be seen as a set of windows through which the userwill interact with the application.In terms of reusability, one application code may be invoked by several interfaces based on different technologies (i.e. a Clibrary used to control an equipment could be invoked either from an OSF/Motif operator interface, or from a C programrunning on a VT100 terminal).A lack of separation between the application and interface software layers leads, in most cases to non-reusable software (i.eequipment access code containing lowlevel OSF/Motif library calls). A functional specification of the data flows betweenthe interface and the application layers is a mandatory step towards better software reusabiblity and a better developmentlifecycle. The HCI development lifecycle described in the next section is a first step in this direction.THE HCI DEVELOPMENT LIFECYCLEAs shown in Figure 4, a typical HCI development lifecycle with XUIMS [6][7] can be decomposed as follows :I. The application concept. This phase, also called the user requirements phase, is aimed at gathering quantifiable HCIrequirements, identifying the future users of the system and drawing the HCI metaphor. II. The functional specification. This phase consists of the translation of an application concept (developed by a user) into afunctional software specification. It should be independent of any particular windowing or graphical system. The

functionality of the application and interface layers should be carefully analysed as well as the data flowing through thesetwo layers. Experience has shown that this phase is very often omitted by developers. This situation leads in most casesto the development of monolithic, windowing-dependent, non-reusable code. III. Prototyping the interface. This exercice is aimed at building a first prototype of the HCI layout with a UIMS. Thebenefits of this phase are the improvement in the definition of the user requirements and the detection of inconsistent orcontradictory requirements. At this stage, no connection between the interface and the application is implemented. IV. Designing the application. This phase consists in the implementation of the application routines (i.e. database access,algorithms, interlocks, ...) as defined in phase I. V. Generating the working application. This phase consists in linking together the interface code generated by the UIMSand the application code in order to produce the working application.Fig 4 : The HCI development lifecycle with XUIMSVery often the HCI lifecycle has to be iterative and prototyping should never be ignored. This XUIMS HCI developmentlifecycle allows the developer to draw the visual metaphor through which the user views and manipulates the system beforestarting any other coding effort.CONCLUSIONSXUIMS is operational since September 1994 and is used by an ever-growing community of software engineers. Majorrejuvenation projects such as the SPS transfer line project and several graphical interfaces for the control of SPS beaminstrumentation and beam transfer have been developed with XUIMS. Off-line software projects like the interface to theSPS and LEP Oracle logging system have also been developed using the XUIMS graphics capabilities. The robustness ofthe end-user applications as well as the openness of the environment encourages us to reduce as much as possible home-made developments and to collaborate with industry. CERN engineers now spend more time on the analysis and less time oncoding. Unfortunately, providing good HCIs remains a difficult task involving detailed technical knowledge (i.e. layering ofthe X-Window system) and concepts of ergonomics. Building a functional specification from user requirements is a crucialphase very often omitted by software developers. By using XUIMS, turning a functional specification into a workingapplication is now a quicker process. Functional Specification Interface Prototyping Application Design Working HCI Interace Design Application Concept

InterfaceCode Generation ApplicationCode Generation

REFERENCES[1] The CERN PS and SL Controls Consolidation Project CERN PS and SL Controls Groups CERN Note PS/91-09 or SL/91-12[2] The CERN SL and ST User Interface Management System - XUIMS Software User Manual. P.Ninin, M.Vanden Eynden CERN SL Note 94-53 (CO)[3] XFaceMaker User�s Guide V3.0. Non Standard Logics[4] XDrawMaker - The Animated Drawing Design Tool for the X Window System. Non Standard Logics[5] The SL X-Window Migration Project Resources Management Policy. M.Tarrant, M.Vanden Eynden CERN SL Note 93-77 (CO)[6] Software Engineering The PSS-05 Way. Quality Systems & Software[7] Software Engineering Standards. C.Mazza, J.Fairclough, B.Melton, D. De Pablo, A.Scheffer, R.Stevens - Prentice Hall� XFaceMaker is a trademark of Non Standard Logics, France.� XDrawMaker is a trademark of Non Standard Logics, France.� XRT/2D, XRT/3D, and XRT/Table are trademarks of KL Group, Inc.