Open Access Front Ends, Models, and Data Acquistion RedirectionKevin CahillFermilabAccelerator Division Controls DepartmentMS 347P.O. Box 500Batavia, IL. 60510 USAThe task of building a front end or embedded model is formidable. The required understanding of data acquisition andnetwork and error-reporting protocols complicate a simple task such as providing a calculated luminosity readback.Models have an additional burden of interfacing to existing programs.This paper describes an architecture which supports the creation of front ends and models. The open access frameworkallows programmers to create clients at a high level of abstraction.HISTORICAL BACKGROUNDA data server in a control system must implement the functionality defined by the data acquisition protocols. Thistypically includes the decomposition of incoming network messages, initiating or canceling requests, scheduling datareturn on a periodic frequency or clock event, construction of network reply frames, error handling and diagnostics to aiddebugging.These details may be overwhelming. Consequently a new data readback summing two channels, for example, are oftenadded to an existing front end that supports a variety of special data types. The disadvantage here is the delay incurred asthe inventor of the channel explains the implementation and waits for the front end support person to code it. Also,delays may occur due to waiting for an opportune time to test the new code which could crash and threaten all the servicesof the front end. Another alternative is to implement a process which sets the calculated value to a channel in an existingfront end. The disadvantage here is the insensitivity to data collection rates. Regardless of the users� interest in fast orslow collection or long periods of disinterest, the calculation and setting of the value proceeds at a constant, fixed rate.OPEN ACCESS FRONT ENDThe open access front end provides an architecture for rapid implementation of a data acquisition server. Further, itprovides the foundation for model implementations.The open access front end architecture consists of processes, database tables, applications, and libraries. The processesinclude the network addressable front end which is responsible for handling the data acquisition protocols, coordination ofclients including their requests and replies, error handling and diagnostics. Other processes are the open access clientswhich are user-written client processes that implement a data acquisition feature. Sybase database tables hold informationregarding named open access clients. Applications include the open access client registration program which manipulatesdatabase registration tables. Library support provides increasing levels of abstraction to the client while supporting thenetwork-based connection to the open access front end.

OPEN ACCESS CLIENTAs an example, suppose one wanted the Julian date available as a device reading. The simplest implementation stepswould include:- adding an open access client description to the database specifying:- the name, node, and class code for the open access client- the open access front end node to serve this client- an abstract of service definition, error code if not connected, and an EMAIL address of the maintainer- creating a database entry for the channel- specifying the class code of the client and appropriate node- creating an open access client- a mainline of one line containing a function call to initialize the open access client stream with client name, and optional reading, setting, periodic, and diagnostic function addresses- a reading function of one line to stuff the Julian date into a passed structure- institutionalize the open access client- submit source to source code capture system- request service initiation to central services group who will create the appropriate command files for starting/stopping the clientThe open access client library offers many services to clients. Synchronous and asynchronous replies are supported.Settings may be echoed to the database. Many process statistics and diagnostics are available to aid debugging. Processmonitoring and transparent reconnection is provided.PROVISIONS FOR TESTINGEven before the open access front end architecture implementation began, the question of how to debug clients arose.Debugging in place is inconvenient to the user community. Creation of similar database entries and clients might alsorequire changes to the driving application to reference the similar database entries. The ability to redirect data acquisitionrequests to a test client offers simplicity as well as support for models.The data acquisition manager supports an API to redirect lists of devices or all datapool requests of an application to openaccess clients under test or to a model or a model under test. A general purpose redirection application and severalspecific model applications provide the user�s interface to redirection. Redirection involves modifying the target front endnode and front end specific addressing information when making a data request. An open access client running on anynode other than its designated client node is considered to be a client under test. After connecting to the test open accessfront end node, any application within the control system may have some or all data acquisition redirected to the testclient. Likewise, data acquisition for a program may be redirected to the model open access front end and its clients or tothe test model open access front end and clients under test.OPEN ACCESS MODELSThe Fermilab accelerator control system actually has two open access front end nodes, one open access model node, oneopen access front end node supporting clients under test and one open access model node supporting clients under test.One of the first model clients to emerge was the MIRROR model. MIRROR establishes a datapool of all channels thathave been redirected, initializes the pool with current readings and settings from the true front end and simply reflects newsettings into the reading pool. If a user initializes a parameter page without redirection, true readings are displayed. If theredirection application redirects all data acquisition for the parameter page application, MIRROR will receive the requests,populate from the real world and the parameter page will begin a static display of unchanging data. The look of theapplication does change as a yellow diagonal line is drawn across the application to indicate redirection. Now, the usermay safely knob devices, turn devices on and off or otherwise test the application in a safe way since settings are simplyreflected into readings within the MIRROR pool. MIRROR provides a safe environment to debug an application�ssettings as well as to explore an unfamiliar page.Another model client is SRFILE. SRFILE establishes one or more datapools initialized with the readings and settingsfrom a save/restore file. Utilizing redirection, any application can contribute to the save/restore system.

LIBRARY SUPPORTWith each development in client or model support, reusable attributes are made available in a public library. SRFILEinherited the internal datapool management created by MIRROR and simply specifies an alternate initial population ofthe internal datapool. Another model is SDASRV, serving up collider fill data identical to SRFILE except for the initialpopulation method. Auto population of a memory-based pool from real data acquisition, database settings, save files, orcollider fill data is exploited by most open access clients and models.Other open access model clients are emerging to support physics modeling of beam lines and operator training.Continued evolution of redirection includes using the save/restore system to support model saves and restores.A dozen open access front end clients exist ranging from PSEUDO, supporting hundreds of devices set by applicationprograms, to SCADA, the control system�s port into a supervisory control and data acquisition system used at the sitepower substation.CONCLUSIONSThe open access front end and client architecture offers the user community easy solutions to data serving needs. Theopen access model and client architecture allows existing applications that use data acquistion to display historical data orto provide application support for model presentations without requiring changes to the application. The redirectioncapabilities in support of models and clients under test is a powerful extension to the data acquisition system. Thissingle, encompassing framework has paid dividends through exploiting reusability to solve multiple problems.ACKNOWLEDGMENTSThe design and implementation of open access front ends, models, clients, supporting applications, and library routinesrepresents the work of many individuals. Brian Hendricks, Bob Joshel, Boris Lublinsky, Junye Wang, and TimZingelman all made significant contributions.